(footprint "SpringContact_Harwin_S1941-46R"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "7.25mm SMT Multi-directional Spring Contact (T+R), https://cdn.harwin.com/pdfs/S1941R.pdf")
	(tags "spring contact emi emc shield")
	(property "Reference" "REF**"
		(at -1 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "SpringContact_Harwin_S1941-46R"
		(at -1 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.1 0)
		(size 4.6 5.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/SpringContact_Harwin_S1941-46R.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
