(footprint "AMASS_XT30PW-M_1x02_P2.50mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Connector XT30 Horizontal PCB Male, https://www.tme.eu/Document/6eb2005a51a52592b3f19e8a450c54c8/XT30PW-M.pdf")
	(tags "RC Connector XT30")
	(property "Reference" "REF**"
		(at -2.5 -14.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "AMASS_XT30PW-M_1x02_P2.50mm_Horizontal"
		(at -2.5 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "-"
		(at 3 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at -8 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at -2.5 -3 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -8 -10)
		(size 1.4 1.4)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 3 -10)
		(size 1.4 1.4)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 3.5 3.5)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.22)
	)
	(pad "2" thru_hole circle
		(at -5 0)
		(size 3.5 3.5)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT30PW-M_1x02_P2.50mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
