(footprint "AMASS_XT60PW-M_1x02_P7.20mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Connector XT60 Horizontal PCB Female, https://www.tme.eu/Document/b13629717d44ae038681dba08d18c0b6/XT60PW-M.pdf")
	(tags "RC Connector XT60")
	(property "Reference" "REF**"
		(at 3.6 -17.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "AMASS_XT60PW-M_1x02_P7.20mm_Horizontal"
		(at 3.6 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "-"
		(at -2.8 2.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at 9.5 2.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 3.6 -3.6 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole rect
		(at -3.15 -6)
		(size 0.9 2)
		(drill oval 0.6 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole rect
		(at 10.35 -6)
		(size 0.9 2)
		(drill oval 0.6 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 4.1 4.1)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 7.2 0)
		(size 4.1 4.1)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT60PW-M_1x02_P7.20mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
