(footprint "AMASS_XT90PW-M_1x02_P10.90mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Connector XT90 Horizontal PCB Male  500V 30A IP40, https://www.bto.pl/pdf/09025/XT90PW-M.pdf")
	(tags "RC")
	(property "Reference" "REF**"
		(at 5.449999 -17.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "AMASS_XT90PW-M_1x02_P10.90mm_Horizontal"
		(at 3.6 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "-"
		(at -4.3 2.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at 14.7 2.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 5.449999 -8.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 7.2 7.2)
		(drill 3.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 10.899998 0)
		(size 7.2 7.2)
		(drill 3.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole rect
		(at -4 -9.4)
		(size 1.6 2.4)
		(drill oval 0.6 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole rect
		(at 14.9 -9.4)
		(size 1.6 2.4)
		(drill oval 0.6 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT90PW-M_1x02_P10.90mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
