(footprint "Amphenol_M8S-03PMMR-SF8001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "M8 Male connector for panel, 90° PCB mount (https://www.amphenolltw.com/2012download/2D%20PDF/03_M%20Series%20Sensor%20Connectors/M8S-XXPMMR-SF8001.pdf)")
	(tags "three-pin M8")
	(property "Reference" "REF**"
		(at -5.6 -8.4 180)
		(layer "F.SilkS")
	)
	(property "Value" "Amphenol_M8S-03PMMR-SF8001"
		(at -8.2 12.2 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -5.6 1.75 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 135)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.95 1.75 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 3.5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 0.5 -4.5 90)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 0.5 8 90)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Amphenol.3dshapes/Amphenol_M8S-03PMMR-SF8001.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
