(footprint "Jack_3.5mm_CUI_SJ-3524-SMT_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
	(tags "3.5mm audio cui horizontal jack stereo")
	(property "Reference" "REF**"
		(at 0 -9.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_CUI_SJ-3524-SMT_Horizontal"
		(at 0 13 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -2.5)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 4.5)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "R" smd rect
		(at 3.7 -1.6)
		(size 2.8 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S" smd rect
		(at -3.7 -3.6)
		(size 2.8 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T" smd rect
		(at -3.7 5.8)
		(size 2.8 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "TN" smd rect
		(at 0.75 9.8)
		(size 2.8 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ-3524-SMT_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
