(footprint "Jack_3.5mm_CUI_SJ1-3514N_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TRS 3.5mm, horizontal, through-hole, with tip switch, https://www.cuidevices.com/product/resource/sj1-351xn.pdf")
	(tags "TRS audio jack stereo horizontal")
	(property "Reference" "REF**"
		(at 5.2 -7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_CUI_SJ1-3514N_Horizontal"
		(at 5.45 7.1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.2 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "R" thru_hole oval
		(at 8.3 -5)
		(size 3 1.5)
		(drill oval 2 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole oval
		(at 0 0 270)
		(size 3.5 2.5)
		(drill oval 2 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole oval
		(at 3.5 4.5)
		(size 3.5 2.5)
		(drill oval 2 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "TN" thru_hole oval
		(at 11.1 4.2 90)
		(size 3.1 2.1)
		(drill oval 2 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3514N_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
