(footprint "Jack_3.5mm_CUI_SJ1-3523N_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
	(tags "TRS audio jack stereo horizontal")
	(property "Reference" "REF**"
		(at 0 -8.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_CUI_SJ1-3523N_Horizontal"
		(at 0 -10 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -2.2 3.5)
		(end -2.2 4.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.2 4.5)
		(end -6.5 4.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.8 3.1)
		(end -1.8 3.1)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 2.2 3.5)
		(end 2.2 4.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 2.2 4.5)
		(end 6.5 4.5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -2.2 3.5)
		(mid -2.082843 3.217158)
		(end -1.8 3.1)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 1.8 3.1)
		(mid 2.082843 3.217157)
		(end 2.2 3.5)
		(layer "Edge.Cuts")
	)
	(fp_text user "PCB edge"
		(at 0 3.65 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5 0)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -5 2.5)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 -5)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5 0)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5 2.5)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "R" thru_hole oval
		(at -5 -5)
		(size 1.2 2.2)
		(drill oval 0.4 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole oval
		(at 0 0)
		(size 2.2 1.2)
		(drill oval 1.4 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole oval
		(at 5 -5 180)
		(size 1.2 2.2)
		(drill oval 0.4 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3523N_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
