(footprint "Jack_3.5mm_CUI_SJ1-3533NG_Horizontal_CircularHoles"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TRS 3.5mm, horizontal, through-hole, , circular holeshttps://www.cui.com/product/resource/sj1-353xng.pdf")
	(tags "TRS audio jack stereo horizontal circular")
	(property "Reference" "REF**"
		(at 0.1 -6.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_CUI_SJ1-3533NG_Horizontal_CircularHoles"
		(at 0.1 14.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.1 3.8 0)
		(layer "F.Fab")
	)
	(pad "R" thru_hole circle
		(at 2 7.9)
		(size 2.8 2.8)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole circle
		(at 0 0)
		(size 2.8 2.8)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole circle
		(at 2 2.4)
		(size 2.8 2.8)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3533NG_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
