(footprint "Jack_3.5mm_KoreanHropartsElec_PJ-320D-4A_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Korean Hroparts Elec PJ-320D-4A (https://datasheet.lcsc.com/lcsc/1810121716_Korean-Hroparts-Elec-PJ-320D-4A_C95562.pdf)")
	(tags "smt female jack horizontal")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_KoreanHropartsElec_PJ-320D-4A_Horizontal"
		(at 0 6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -4.75 0)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.25 0)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "R1" smd rect
		(at -0.15 -3.25)
		(size 1.2 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd rect
		(at -3.15 -3.25)
		(size 1.2 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S" smd rect
		(at 4.95 3.25)
		(size 1.2 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T" smd rect
		(at 3.85 -3.25)
		(size 1.2 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_KoreanHropartsElec_PJ-320D-4A_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
