(footprint "Jack_3.5mm_Ledino_KB3SPRS_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.reichelt.de/index.html?ACTION=7&LA=3&OPEN=0&INDEX=0&FILENAME=C160%252FKB3SPRS.pdf")
	(tags "jack stereo TRS")
	(property "Reference" "REF**"
		(at -3.5 2.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_Ledino_KB3SPRS_Horizontal"
		(at 2.3 -12.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.7 -4.6 0)
		(layer "F.Fab")
	)
	(pad "R" thru_hole oval
		(at 4.1 -9.8)
		(size 4 2.2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "RN" thru_hole oval
		(at 2.9 -7.1)
		(size 4 2.2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole oval
		(at -3.9 -4.6)
		(size 2.2 4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole rect
		(at 0 0)
		(size 4 2.2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "TN" thru_hole oval
		(at 7.3 -0.5 90)
		(size 4 2.2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_Ledino_KB3SPRS_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
