(footprint "Jack_3.5mm_Lumberg_1503_03_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TRS 3.5mm, horizontal, Surface Mount (SMT), https://downloads.lumberg.com/datenblaetter/en/1503_03.pdf")
	(tags "TRS audio jack horizontal")
	(property "Reference" "REF**"
		(at 3.5 8.68 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_Lumberg_1503_03_Horizontal"
		(at 0 10.14 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.04 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -2.75)
		(size 1.3 1.3)
		(drill 1.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 3.55)
		(size 1.3 1.3)
		(drill 1.3)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "MP" smd roundrect
		(at -4.25 -1.75)
		(size 2.2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "MP" smd roundrect
		(at 4.25 -1.75)
		(size 2.2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "R" smd roundrect
		(at 3.65 5)
		(size 2 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1315789474)
	)
	(pad "S" smd roundrect
		(at -3.65 5)
		(size 2 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1315789474)
	)
	(pad "T" smd roundrect
		(at 0 7.85)
		(size 2 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1315789474)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_Lumberg_1503_03_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
