(footprint "Jack_3.5mm_Lumberg_1503_07_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TRS 3.5mm, horizontal, through-hole, height 5mm, width 6.5mm, https://downloads.lumberg.com/datenblaetter/en/1503_07.pdf")
	(tags "TRS audio jack horizontal")
	(property "Reference" "REF**"
		(at 2.85 -7.3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_Lumberg_1503_07_Horizontal"
		(at 2.8 10 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.85 1.025 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0.35 3.5)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.35 3.5)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "R" thru_hole oval
		(at 5.15 7.5)
		(size 1.8 2.3)
		(drill oval 0.8 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole oval
		(at 0.55 7.5)
		(size 1.8 2.3)
		(drill oval 0.8 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole oval
		(at 0 0)
		(size 2 2.3)
		(drill oval 1 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole oval
		(at 5.7 0)
		(size 2 2.3)
		(drill oval 1 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_Lumberg_1503_07_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
