(footprint "Jack_3.5mm_PJ311_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PJ311 6pin SMD 3.5mm stereo headphones jack.")
	(tags "headphones jack plug stereo 3.5mm PJ311")
	(property "Reference" "REF**"
		(at 0 -10.16 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_PJ311_Horizontal"
		(at 0 7.17 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -4.3)
		(size 1.5 1.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 2.7)
		(size 1.5 1.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -3.5 -4.7)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.5 -4.7)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.5 -1.3)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.5 2.5)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 3.5 4.7)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.5 4.2)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_PJ311_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
