(footprint "Jack_3.5mm_PJ320D_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320D-72.html)")
	(tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
	(property "Reference" "REF**"
		(at 0.05 -5.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_PJ320D_Horizontal"
		(at -0.025 6.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -1.195 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -4.775 0)
		(size 1.5 1.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.225 0)
		(size 1.5 1.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "R1" smd rect
		(at -0.175 -3.25)
		(size 1.2 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd rect
		(at -3.175 -3.25)
		(size 1.2 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S" smd rect
		(at 4.925 3.25)
		(size 1.2 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T" smd rect
		(at 3.825 -3.25)
		(size 1.2 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320D_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
