(footprint "Jack_3.5mm_PJ320E_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320E-177.html)")
	(tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
	(property "Reference" "REF**"
		(at 2.54 -13.97 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_PJ320E_Horizontal"
		(at 2.54 5.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 -13.97 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 2.3 -5.7 270)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.3 1.3 270)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" thru_hole oval
		(at 5.5 -7 270)
		(size 2 1.4)
		(drill oval 1.2 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R1" thru_hole oval
		(at 0 -4 270)
		(size 2 1.4)
		(drill oval 1.2 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R2" thru_hole oval
		(at 0 -7 270)
		(size 2 1.4)
		(drill oval 1.2 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole oval
		(at 4.5 1.5 270)
		(size 2 1.4)
		(drill oval 1.2 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole rect
		(at 0 0 270)
		(size 2 1.4)
		(drill oval 1.2 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320E_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
