(footprint "Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
	(tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
	(property "Reference" "REF**"
		(at -4.03 1.08 180)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles"
		(at 0 5 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "KEEPOUT"
		(at 0 6.48 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 8 180)
		(layer "F.Fab")
	)
	(pad "S" thru_hole rect
		(at 0 0 180)
		(size 1.93 1.83)
		(drill 1.22)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole circle
		(at 0 11.4 180)
		(size 2.13 2.13)
		(drill 1.43)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "TN" thru_hole circle
		(at 0 3.1 180)
		(size 2.13 2.13)
		(drill 1.42)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 1.505141 6.48) (xy 1.48493 6.234171) (xy 1.424841 5.994945) (xy 1.326486 5.768744) (xy 1.192508 5.561645)
				(xy 1.026504 5.37921) (xy 0.832932 5.226336) (xy 0.616992 5.107131) (xy 0.384482 5.024794) (xy 0.141646 4.981539)
				(xy -0.104993 4.978525) (xy -0.348813 5.015835) (xy -0.583266 5.092466) (xy -0.802054 5.20636) (xy -0.999303 5.354458)
				(xy -1.169714 5.532784) (xy -1.308712 5.736548) (xy -1.412564 5.960278) (xy -1.478481 6.197965)
				(xy -1.504692 6.443226) (xy -1.490493 6.689475) (xy -1.436266 6.930099) (xy -1.343468 7.158634)
				(xy -1.214589 7.368945) (xy -1.053092 7.555382) (xy -0.863313 7.712939) (xy -0.65035 7.837385) (xy -0.419921 7.925377)
				(xy -0.178215 7.974553) (xy 0.068278 7.983592) (xy 0.312936 7.95225) (xy 0.549191 7.88137) (xy 0.770697 7.772856)
				(xy 0.971505 7.629621) (xy 1.146223 7.455512) (xy 1.290158 7.255205) (xy 1.399445 7.034079) (xy 1.471149 6.798074)
				(xy 1.503344 6.553526)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
