(footprint "Jack_3.5mm_Technik_TWP-3002_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3.5mm Horizontal Waterproof Stereo Headphones Jack, https://www.technik.com.hk/images/pdf_product/WP3002-PA66-A.pdf")
	(tags "audio jack stereo horizontal waterproof")
	(property "Reference" "REF**"
		(at -4.6 -10.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_Technik_TWP-3002_Horizontal"
		(at -4.5 3.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -4.5 -1.9 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole oval
		(at -9 -3.8)
		(size 1.9 1)
		(drill oval 1.4 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole oval
		(at -9 0)
		(size 1.9 1)
		(drill oval 1.4 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" np_thru_hole circle
		(at -4.05 -7.8)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "R1" thru_hole oval
		(at 0 -1.9)
		(size 1 1.9)
		(drill oval 0.5 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R2" thru_hole oval
		(at 0 -5.1)
		(size 1.9 1)
		(drill oval 1.4 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole oval
		(at 0 1.3)
		(size 1.9 1)
		(drill oval 1.4 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole oval
		(at 0 -3.8)
		(size 1.9 1)
		(drill oval 1.4 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole oval
		(at 0 0)
		(size 1.9 1)
		(drill oval 1.4 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_Technik_TWP-3002_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
