(footprint "Jack_6.35mm_Neutrik_NJ6TB-V_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "6.35mm (1/4 in) Vertical Jack, 3 x switching (normalling) stereo jack  B-gauge type (T/TN/R/RN/S/SN), https://www.neutrik.com/en/product/nj6tb-v")
	(tags "neutrik jack vertical")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_6.35mm_Neutrik_NJ6TB-V_Vertical"
		(at 0 14.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 5.72 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.18 12.07 180)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.81 1.91 180)
		(size 2.1 2.1)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "R" thru_hole circle
		(at 5.08 5.72 180)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "RN" thru_hole circle
		(at 4.45 10.17 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole circle
		(at -5.08 5.72 180)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SN" thru_hole circle
		(at -4.45 10.17 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole circle
		(at 0 0 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "TN" thru_hole circle
		(at -5.08 0.64 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_6.35mm_Neutrik_NJ6TB-V_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
