(footprint "Jack_6.35mm_Neutrik_NMJ6HHD2_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with half threaded nose and offset PCB pins, https://www.neutrik.com/en/product/nmj6hhd2")
	(tags "neutrik jack m")
	(property "Reference" "REF**"
		(at 6.35 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_6.35mm_Neutrik_NMJ6HHD2_Horizontal"
		(at 6.35 19 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 6.35 8.115 0)
		(layer "F.Fab")
	)
	(pad "R" thru_hole circle
		(at 6.35 0)
		(size 3 3)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "RN" thru_hole circle
		(at 6.35 16.23)
		(size 3 3)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole circle
		(at 12.7 0)
		(size 3 3)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SN" thru_hole circle
		(at 12.7 16.23)
		(size 3 3)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "TN" thru_hole circle
		(at 0 16.23)
		(size 3 3)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_6.35mm_Neutrik_NMJ6HHD2_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
