(footprint "Jack_XLR-6.35mm_Neutrik_NCJ6FA-H-0_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, horizontal PCB mount, retention spring, https://www.neutrik.com/en/product/ncj6fa-h-0")
	(tags "neutrik jack combo a")
	(property "Reference" "REF**"
		(at 9.015 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_XLR-6.35mm_Neutrik_NCJ6FA-H-0_Horizontal"
		(at 9.015 21 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 15.265 6.985 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 8.89 6.985)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12.065 1.27)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12.065 12.7)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -0.635 13.97)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -5.08 6.985)
		(size 2.7 2.7)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G" thru_hole circle
		(at 11.43 -1.27)
		(size 3.2 3.2)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R" thru_hole circle
		(at -4.445 9.8425)
		(size 2.7 2.7)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole circle
		(at -4.445 4.1275)
		(size 2.7 2.7)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole circle
		(at 2.54 2.54)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole circle
		(at 2.54 11.43)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_XLR-6.35mm_Neutrik_NCJ6FA-H-0_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
