(footprint "Jack_XLR-6.35mm_Neutrik_NCJ9FI-V_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack, vertical PCB mount, retention spring, https://www.neutrik.com/en/product/ncj9fi-v")
	(tags "neutrik jack combo i")
	(property "Reference" "REF**"
		(at -6.15 -14 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_XLR-6.35mm_Neutrik_NCJ9FI-V_Vertical"
		(at -6.15 18 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -6.15 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -12.3 0)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -6.15 6.05)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G" thru_hole circle
		(at -6.15 10.45)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R" thru_hole circle
		(at -0.35 5.8)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "RN" thru_hole circle
		(at -3.15 3)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole circle
		(at -11.95 5.8)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SN" thru_hole circle
		(at -9.15 3)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole circle
		(at -11.35 -5.2)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "TN" thru_hole circle
		(at -9.15 -3)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_XLR-6.35mm_Neutrik_NCJ9FI-V_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
