(footprint "Jack_XLR_Neutrik_NC3FAHL1-0_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral left PCB mount, retention spring instead of latch, https://www.neutrik.com/en/product/nc3fahl1-0")
	(tags "neutrik xlr a")
	(property "Reference" "REF**"
		(at 3.81 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_XLR_Neutrik_NC3FAHL1-0_Horizontal"
		(at 3.81 20 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_line
		(start -8.89 10.79)
		(end -8.89 15.87)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.54 10.79)
		(end -8.89 10.79)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.54 15.87)
		(end -2.54 10.79)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 16.61 15.87)
		(end -8.99 15.87)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 3.81 13.52 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 9.52 7.61)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3.81 -3.18)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 7.62 0)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_XLR_Neutrik_NC3FAHL1-0_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
