(footprint "Jack_XLR_Neutrik_NC3MBH-E_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, horizontal PCB mount, additional ground contacts, https://www.neutrik.com/en/product/nc3mbh-e")
	(tags "neutrik xlr b")
	(property "Reference" "REF**"
		(at 3.81 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_XLR_Neutrik_NC3MBH-E_Horizontal"
		(at 3.81 22 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.81 15.43 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 8.89)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.62 13.97)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.62 0)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 3.81 0)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G" thru_hole circle
		(at 3.81 5.08)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_XLR_Neutrik_NC3MBH-E_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
