(footprint "Jack_XLR_Neutrik_NC3MBHR-B_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, lateral right PCB mount, black chrome shell, https://www.neutrik.com/en/product/nc3mbhr-b")
	(tags "neutrik xlr b")
	(property "Reference" "REF**"
		(at 9.39 -10 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_XLR_Neutrik_NC3MBHR-B_Horizontal"
		(at 9.39 18 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_line
		(start 12.7 10.16)
		(end 12.7 16.51)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.7 16.51)
		(end 17.78 16.51)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 17.78 -8.99)
		(end 17.78 16.61)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 17.78 10.16)
		(end 12.7 10.16)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 15.43 3.81 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 10.78 3.81)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 3.81)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 7.62)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "G" thru_hole circle
		(at 5.08 3.81)
		(size 2.9 2.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_XLR_Neutrik_NC3MBHR-B_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
