(footprint "Jack_speakON-6.35mm_Neutrik_NLJ2MDXX-H_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "speakON Combo, 2 pole combination of speakON socket and 6.35mm (1/4in) jack receptacle, horizontal pcb mount, replaces NLJ2MD-H, https://www.neutrik.com/en/product/nlj2mdxx-h")
	(tags "neutrik speakon combo")
	(property "Reference" "REF**"
		(at 17.5 -11 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_speakON-6.35mm_Neutrik_NLJ2MDXX-H_Horizontal"
		(at 17.5 17.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 17.5 4.765 0)
		(layer "F.Fab")
	)
	(pad "1+" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1-" thru_hole circle
		(at 4.44 9.53)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_speakON-6.35mm_Neutrik_NLJ2MDXX-H_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
