(footprint "Jack_speakON_Neutrik_NL4MDXX-V_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, countersunk thru holes, vertical PCB mount, replaces NL4MD-V, NL4MD-V-R, NL4MD-V-S, https://www.neutrik.com/en/product/nl4mdxx-v")
	(tags "neutrik speakon")
	(property "Reference" "REF**"
		(at 0.7 -13 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_speakON_Neutrik_NL4MDXX-V_Vertical"
		(at 0.7 20.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.7 3.6 0)
		(layer "F.Fab")
	)
	(pad "1+" thru_hole circle
		(at 0 0)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1-" thru_hole circle
		(at -4.7 2.9)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2+" thru_hole circle
		(at 0 7.2)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2-" thru_hole circle
		(at 6.1 4.3)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_speakON_Neutrik_NL4MDXX-V_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
