(footprint "Plug_3.5mm_CUI_SP-3541"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4 contacts, 3.5mm audio plug, https://www.cuidevices.com/product/resource/pdf/sp-3541.pdf")
	(tags "3.5mm plug TRRS")
	(property "Reference" "REF**"
		(at 0 8.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Plug_3.5mm_CUI_SP-3541"
		(at 0.75 9.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -0.05 1.15 0)
		(layer "F.Fab")
	)
	(pad "R1" thru_hole roundrect
		(at 0 3.6)
		(size 2.5 1.3)
		(drill oval 1.5 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "R2" thru_hole roundrect
		(at 0 1.9)
		(size 2.5 1.3)
		(drill oval 1.5 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "S" thru_hole roundrect
		(at 0 0)
		(size 2.5 1.3)
		(drill oval 1.5 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "T" thru_hole roundrect
		(at 0 5.3)
		(size 2.5 1.3)
		(drill oval 1.5 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Plug_3.5mm_CUI_SP-3541.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
