(footprint "BarrelJack_CLIFF_FC681465S_SMT_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Surface-mount DC Barrel Jack, https://www.cliffuk.co.uk/products/dcconnectors/FC681465S.pdf")
	(tags "Power Jack SMT")
	(property "Reference" "REF**"
		(at -6.5 6.5 180)
		(layer "F.SilkS")
	)
	(property "Value" "BarrelJack_CLIFF_FC681465S_SMT_Horizontal"
		(at -0.5 8.5 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.5 0.5 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole oval
		(at -2.9 0 90)
		(size 2 1.5)
		(drill oval 2 1.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.5 0 90)
		(size 2 2)
		(drill 2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -3 -5.5 90)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 3 -5.5 90)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3 5.5 90)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3 5.5 90)
		(size 3 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_CLIFF_FC681465S_SMT_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
