(footprint "BarrelJack_CUI_PJ-079BH_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Barrel Jack, 2.5mm ID, 5.5mm OD, 24V, 5A, switch, https://www.cui.com/product/resource/pj-079bh.pdf ")
	(tags "barrel jack cui dc power")
	(property "Reference" "REF**"
		(at -9.8 -2.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "BarrelJack_CUI_PJ-079BH_Horizontal"
		(at -3.6 11.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -4.5 4.3 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.2 6.3 180)
		(size 2.13 2.13)
		(drill 2.13)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 1.8 3)
		(drill oval 0.8 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at -8.5 0 180)
		(size 1.8 3)
		(drill oval 0.8 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at -3.2 0 180)
		(size 1.8 3)
		(drill oval 0.8 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -9.4 7.3 180)
		(size 1.6 3)
		(drill oval 0.6 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 0.4 7.3 180)
		(size 1.6 3)
		(drill oval 0.6 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-079BH_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
