(footprint "BarrelJack_Kycon_KLDX-0202-xC_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DC Barrel Jack 2mm or 2.5mm center pin, https://www.kycon.com/Pub_Eng_Draw/KLDX-0202-AC%20&%20BC.pdf")
	(tags "power jack 2mm 2.5mm KLDX-0202-BC KLDX-0202-AC")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "BarrelJack_Kycon_KLDX-0202-xC_Horizontal"
		(at -6 7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -2.9 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 4.5)
		(drill oval 1 3.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at -6.2 0)
		(size 2 4)
		(drill oval 1 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at -3.2 4.7 90)
		(size 2 4)
		(drill oval 1 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Kycon_KLDX-0202-xC_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
