(footprint "BarrelJack_SwitchcraftConxall_RAPC10U_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DC Power Jack, 13A, 24V, Panel Mount,Through-hole, https://www.switchcraft.com/Drawings/RAPC10U_CD.pdf")
	(tags "barreljack switchcraftconxall dc power")
	(property "Reference" "REF**"
		(at -10.8 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "BarrelJack_SwitchcraftConxall_RAPC10U_Horizontal"
		(at -11 9.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_line
		(start -18.67 -9)
		(end -18.67 9)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at -10.4 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.02 5.02)
		(drill oval 1.02 4.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at -5.18 0)
		(size 2.02 5.02)
		(drill oval 1.02 4.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_SwitchcraftConxall_RAPC10U_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
