(footprint "BarrelJack_Wuerth_694103107102_1.35x3.9mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Wuerth Elektronik barrel jack connector, SMD, 3.9mm OD, 1.35mm ID, with switch, 18V, 5A, dimensions: 9.3 x 8 x 5.3 mm (L x W x H), datasheet: https://www.we-online.com/components/products/datasheet/694103107102.pdf")
	(tags "barrel jack Wuerth Elektronik 694103107102")
	(property "Reference" "REF**"
		(at -6.57 3.01 90)
		(layer "F.SilkS")
	)
	(property "Value" "BarrelJack_Wuerth_694103107102_1.35x3.9mm"
		(at 0 5.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" "https://www.we-online.com/components/products/datasheet/694103107102.pdf"
		(at 0 -0.205 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 -0.205 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -3.15 180)
		(size 1 1)
		(drill 1)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 1.85 180)
		(size 1 1)
		(drill 1)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at 4.3 -1.15 270)
		(size 2.2 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1136363636)
	)
	(pad "1" smd roundrect
		(at 4.3 3.35 270)
		(size 2.2 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1136363636)
	)
	(pad "2" smd roundrect
		(at -4.3 -1.15 270)
		(size 2.2 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1136363636)
	)
	(pad "3" smd roundrect
		(at -4.3 3.35 270)
		(size 2.2 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1136363636)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Wuerth_694103107102_1.35x3.9mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
