(footprint "BarrelJack_Wuerth_694106106102_2.0x5.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Wuerth Elektronik 694106106102 Barrel Jack, 2.0x5.5mm, https://www.we-online.com/components/products/datasheet/694106106102.pdf")
	(tags "barrel jack Wuerth Elektronik 694106106102")
	(property "Reference" "REF**"
		(at -3.17 -6.725 0)
		(layer "F.SilkS")
	)
	(property "Value" "BarrelJack_Wuerth_694106106102_2.0x5.5mm"
		(at 0.05 9.605 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.01 0.655 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -1.425)
		(size 1.8 1.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 3.075)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -5.5 -3.075)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "1" smd roundrect
		(at -5.5 3.075)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "2" smd roundrect
		(at 5.5 3.075)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "3" smd roundrect
		(at 5.5 -3.075)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Wuerth_694106106102_2.0x5.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
