(footprint "CF-Card_3M_N7E50-A516xx-30"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Compact Flash Card connector, polarization inverse (https://multimedia.3m.com/mws/media/22424O/3mtm-cf-card-header-type-i-low-profile-surface-mount-ts0747.pdf)")
	(tags "connector cf")
	(property "Reference" "REF**"
		(at 7.22 0 90)
		(layer "F.SilkS")
	)
	(property "Value" "CF-Card_3M_N7E50-A516xx-30"
		(at 10.39 0 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.535 0 90)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -0.1 -19.37 90)
		(size 3.99 3.99)
		(drill 2.21)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -0.1 19.37 90)
		(size 3.99 3.99)
		(drill 2.21)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" smd rect
		(at 2.57 -23.34 90)
		(size 2.49 4.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.57 23.34 90)
		(size 2.49 4.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" np_thru_hole circle
		(at 2.9 -19.37 90)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.9 19.37 90)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -3.1 -15.56 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.1 -14.29 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.1 -13.02 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.1 -11.75 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.1 -10.48 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.1 -9.21 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.1 -7.94 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.1 -6.67 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.1 -5.4 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -3.1 -4.13 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.1 -2.86 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.1 -1.59 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -3.1 -0.32 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -3.1 0.95 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -3.1 2.22 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -3.1 3.49 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -3.1 4.76 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -3.1 6.03 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -3.1 7.3 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -3.1 8.57 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -3.1 9.84 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -3.1 11.11 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -3.1 12.38 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -3.1 13.65 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -3.1 14.92 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -3.1 -14.92 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -3.1 -13.65 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -3.1 -12.38 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -3.1 -11.11 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -3.1 -9.84 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -3.1 -8.57 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -3.1 -7.3 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -3.1 -6.03 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at -3.1 -4.76 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -3.1 -3.49 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -3.1 -2.22 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -3.1 -0.95 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at -3.1 0.32 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -3.1 1.59 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at -3.1 2.86 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -3.1 4.13 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at -3.1 5.4 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -3.1 6.67 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -3.1 7.94 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -3.1 9.21 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at -3.1 10.48 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -3.1 11.75 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at -3.1 13.02 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at -3.1 14.29 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at -3.1 15.56 90)
		(size 0.41 3.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/CF-Card_3M_N7E50-A516xx-30.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
