(footprint "SD-SIM_microSD-microSIM_Molex_104168-1620"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "microSD and microSIM connector, https://www.molex.com/pdm_docs/sd/1041681620_sd.pdf")
	(tags "Combo Connector microSD and microSIM")
	(property "Reference" "REF**"
		(at 0 -10.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "SD-SIM_microSD-microSIM_Molex_104168-1620"
		(at 0 11.425 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "C1" smd roundrect
		(at 6.95 -4.525)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "C2" smd roundrect
		(at 6.95 0.035)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "C3" smd roundrect
		(at 6.95 0.915)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "C4" smd roundrect
		(at 6.95 2.675)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "C5" smd roundrect
		(at -6.95 2.675)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "C6" smd roundrect
		(at -6.95 0.915)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "C7" smd roundrect
		(at -6.95 0.035)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "C8" smd roundrect
		(at -6.95 -4.525)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S1" smd roundrect
		(at 6.95 5.315)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S2" smd roundrect
		(at 6.95 4.435)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S3" smd roundrect
		(at -6.95 4.435)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S4" smd roundrect
		(at -6.95 5.315)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S5" smd roundrect
		(at 6.95 1.795)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S6" smd roundrect
		(at 6.95 3.555)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S7" smd roundrect
		(at -6.95 3.555)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S8" smd roundrect
		(at -6.95 1.795)
		(size 1 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" smd roundrect
		(at -6.925 -7.825)
		(size 1.05 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" smd roundrect
		(at -6.925 -3.015)
		(size 1.05 1.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" smd roundrect
		(at -6.925 -1.175)
		(size 1.05 1.34)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" thru_hole custom
		(at -6.455 7.875)
		(size 0.5 1.4)
		(drill oval 0.4 1.3)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.4 -0.4) (xy 0 -0.4) (xy 0 -0.85) (xy -0.65 -0.85) (xy -0.65 0.85) (xy 0 0.85) (xy 0 0.4)
					(xy 0.4 0.4)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.05 0.4)
				(end 0.4 0.4)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.05 -0.4)
				(end 0.4 -0.4)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "SH" thru_hole custom
		(at 6.455 7.875)
		(size 0.5 1.4)
		(drill oval 0.4 1.3)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4 -0.4) (xy 0 -0.4) (xy 0 -0.85) (xy 0.65 -0.85) (xy 0.65 0.85) (xy 0 0.85) (xy 0 0.4) (xy -0.4 0.4)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.05 0.4)
				(end 0.5 0.4)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.05 -0.4)
				(end 0.5 -0.4)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "SH" smd roundrect
		(at 6.925 -7.825)
		(size 1.05 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" smd roundrect
		(at 6.925 -3.015)
		(size 1.05 1.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" smd roundrect
		(at 6.925 -1.175)
		(size 1.05 1.34)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SW" smd roundrect
		(at -6.65 -5.94)
		(size 1.2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -5.99 -8.725) (xy 5.99 -8.725) (xy 5.99 8.965) (xy -5.99 8.965)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/SD-SIM_microSD-microSIM_Molex_104168-1620.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
