(footprint "SD_Card_Device_16mm_SlotDepth"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SD card device PCB layout, contacts and mechanicalm, 16mm slot depth. Manufacture with PCB thickness of 1.4mm, http://www.convict.lu/pdf/ProdManualSDCardv1.9.pdf")
	(tags "SD Card")
	(property "Reference" "REF**"
		(at 9.6 -1.05 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "SD_Card_Device_16mm_SlotDepth"
		(at 0.05 17 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 17.55 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -12 -0.05)
		(end -12 -15)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11 -16)
		(end 7.792893 -16)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 8.146447 -15.853553)
		(end 11.853554 -12.146446)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.25 -6)
		(end 11.25 -4.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.25 -4.5)
		(end 12 -4.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12 -11.792893)
		(end 12 -6)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12 -6)
		(end 11.25 -6)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12 -4.5)
		(end 12 -0.05)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -12 -15)
		(mid -11.707107 -15.707107)
		(end -11 -16)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 7.792893 -16)
		(mid 7.984235 -15.96194)
		(end 8.146447 -15.853553)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 11.853554 -12.146446)
		(mid 11.96194 -11.984234)
		(end 12 -11.792893)
		(layer "Edge.Cuts")
	)
	(fp_text user "PCB Thickness 1.4mm"
		(at -11.7 -0.5 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Write Protect Notch"
		(at -11 -5.1 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" connect roundrect
		(at 6.875 -12.7)
		(size 1.4 3.4)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.07142857143)
		(clearance 0.05)
	)
	(pad "2" connect roundrect
		(at 4.375 -12.7)
		(size 1.4 3.4)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.07142857143)
		(clearance 0.05)
	)
	(pad "3" connect roundrect
		(at 1.875 -12.8)
		(size 1.4 3.6)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.07142857143)
		(clearance 0.05)
	)
	(pad "4" connect roundrect
		(at -0.625 -12.8)
		(size 1.4 3.6)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.07142857143)
		(clearance 0.05)
	)
	(pad "5" connect roundrect
		(at -3.125 -12.7)
		(size 1.4 3.4)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.07142857143)
		(clearance 0.05)
	)
	(pad "6" connect roundrect
		(at -5.625 -12.7)
		(size 1.4 3.4)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.07142857143)
		(clearance 0.05)
	)
	(pad "7" connect roundrect
		(at -8.05 -12.7)
		(size 1.1 3.4)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.07142857143)
		(clearance 0.05)
	)
	(pad "8" connect roundrect
		(at -9.75 -12.7)
		(size 0.9 3.4)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.07142857143)
		(clearance 0.05)
	)
	(pad "9" connect roundrect
		(at 9.375 -10.4)
		(size 1.4 3.4)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.07142857143)
		(clearance 0.05)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -11.95 -10.85) (xy 7.55 -10.85) (xy 7.55 -8.55) (xy 11.95 -8.55) (xy 11.95 -6.05) (xy 11.2 -6.05)
				(xy 11.2 -4.45) (xy 11.95 -4.45) (xy 11.95 -0.1) (xy -11.95 -0.1)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/SD_Card_Device_16mm_SlotDepth.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
