(footprint "SD_Hirose_DM1AA_SF_PEJ82"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SD, SMD, top-mount, push-push (https://www.hirose.com/product/document?clcode=CL0609-0004-8-82&productname=DM1AA-SF-PEJ(82)&series=DM1&documenttype=2DDrawing&lang=en&documentid=0000915301)")
	(tags "SD card connector")
	(property "Reference" "REF**"
		(at 0 -17.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "SD_Hirose_DM1AA_SF_PEJ82"
		(at -0.6 10.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -11.9 -12.75)
		(size 1.3 1.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10.5 -12.75)
		(size 1.3 1.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at 6.075 -14.95)
		(size 1.1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.575 -14.95)
		(size 1.1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.075 -14.95)
		(size 1.1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.425 -14.95)
		(size 1.1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.925 -14.95)
		(size 1.1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -6.425 -14.95)
		(size 1.1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.85 -14.95)
		(size 1.1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -10.55 -14.95)
		(size 1.1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 8.575 -14.95)
		(size 1.1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "CP" smd rect
		(at -13.6 -3.55)
		(size 2 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -14.5 -8.2)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -14.5 10.45)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 14.5 -8.2)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 14.5 10.45)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SW" smd rect
		(at -13.6 8)
		(size 2 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "WP" smd rect
		(at -13.6 5.4)
		(size 2 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/SD_Hirose_DM1AA_SF_PEJ82.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
