(footprint "SD_Kyocera_145638009211859+"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SD Card Connector, Normal Type, Outer Tail, Without Ejector (https://global.kyocera.com/prdct/electro/product/pdf/5638.pdf)")
	(tags "sd card smt")
	(property "Reference" "REF**"
		(at 0 -15.04 180)
		(layer "F.SilkS")
	)
	(property "Value" "SD_Kyocera_145638009211859+"
		(at 0 -0.3 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Copper Keep Out"
		(at 0 -3.4 180)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.7 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -12.1 -5.3 180)
		(size 1.5 1.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12.1 -5.3 180)
		(size 1.5 1.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at 6.88 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "2" smd roundrect
		(at 4.38 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "3" smd roundrect
		(at 1.08 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "4" smd roundrect
		(at -0.62 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "5" smd roundrect
		(at -3.12 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "6" smd roundrect
		(at -5.62 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "7" smd roundrect
		(at -8.05 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "8" smd roundrect
		(at -9.75 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "9" smd roundrect
		(at 9.38 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "10" smd roundrect
		(at 2.68 -12.5)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.313)
	)
	(pad "11" smd roundrect
		(at -13.24 -12.5)
		(size 0.7 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.357)
	)
	(pad "12" smd roundrect
		(at 13.2 8.7)
		(size 1.8 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.139)
	)
	(pad "13" smd roundrect
		(at -13.25 9.9)
		(size 1.7 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.147)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/SD_Kyocera_145638009211859+.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
