(footprint "microSD_HC_Hirose_DM3BT-DSF-PEJS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Micro SD, SMD, reverse on-board, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3BT-DSF-PEJS/category/Drawing%20(2D)/doc_file_id/44097/?file_category_id=6&item_id=06090029900&is_series=)")
	(tags "Micro SD")
	(property "Reference" "REF**"
		(at 0.425 -9.525 0)
		(layer "F.SilkS")
	)
	(property "Value" "microSD_HC_Hirose_DM3BT-DSF-PEJS"
		(at 0.425 9.575 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "KEEPOUT"
		(at 6.85 -3.25 90)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.325 1.575 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.775 -7.625)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.675 -7.625)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.575 -7.625)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.525 -7.625)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.625 -7.625)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.725 -7.625)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3.825 -7.625)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.925 -7.625)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 5.875 -7.725)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 6.725 2.775)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -6.575 7.375)
		(size 1.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -5.825 7.825 45)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -5.575 8.075)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -4.675 -7.625)
		(size 1 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 6.725 -3.425)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 6.725 6.375)
		(size 1.2 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 6.475 -4.025) (xy 7.225 -4.025) (xy 7.225 -7.275) (xy 6.475 -7.275)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 6.475 0.775) (xy 7.225 0.775) (xy 7.225 -2.825) (xy 6.475 -2.825)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3BT-DSF-PEJS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
