(footprint "microSD_HC_Wuerth_693072010801"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://katalog.we-online.de/em/datasheet/693072010801.pdf")
	(tags "Micro SD Wuerth Wurth Würth")
	(property "Reference" "REF**"
		(at 0 -7.99 0)
		(layer "F.SilkS")
	)
	(property "Value" "microSD_HC_Wuerth_693072010801"
		(at 0 9.22 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.15 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.2 -1.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.1 -1.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1 -1.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.1 -1.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.2 -1.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.3 -1.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3.4 -1.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.5 -1.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -6.875 -4.15)
		(size 1.45 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -6.875 4.15)
		(size 1.45 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 6.875 -4.15)
		(size 1.45 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 6.875 4.15)
		(size 1.45 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/microSD_HC_Wuerth_693072010801.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
