(footprint "BNC_Win_364A2x95_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Dual front isolated BNC plug (https://www.winconn.com/wp-content/uploads/364A2595.pdf)")
	(tags "Dual BNC Horizontal Isolated")
	(property "Reference" "REF**"
		(at 0 4.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "BNC_Win_364A2x95_Horizontal"
		(at 0 6.15 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 -0.1 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 0 -2.54)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at -5.08 -8.89)
		(size 3.5 7)
		(drill 2.01)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -2.54 0)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5.08 -8.89)
		(size 3.5 7)
		(drill 2.01)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_Win_364A2x95_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
