(footprint "CoaxialSwitch_Hirose_MS-156C3_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Subminiature Coaxial Switch 1.35mm High, DC to 11GHz")
	(tags "Switch Coaxial RF")
	(property "Reference" "REF**"
		(at 0 -2.4 180)
		(layer "F.SilkS")
	)
	(property "Value" "CoaxialSwitch_Hirose_MS-156C3_Horizontal"
		(at 0 2.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "No Traces"
		(at 0 0 0)
		(layer "Cmts.User")
	)
	(fp_text user "No Resist"
		(at 0 0.4 0)
		(layer "Cmts.User")
	)
	(fp_text user "KEEPOUT"
		(at 0 -0.5 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1 0 180)
		(size 0.3 0.4)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "" smd rect
		(at -0.7 -1 180)
		(size 0.4 0.4)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "" smd rect
		(at -0.7 1 180)
		(size 0.4 0.4)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "" smd rect
		(at 0 -0.8 180)
		(size 0.5 0.3)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "" smd rect
		(at 0 0.8 180)
		(size 0.5 0.3)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "" smd rect
		(at 0.7 -1 180)
		(size 0.4 0.4)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "" smd rect
		(at 0.7 1 180)
		(size 0.4 0.4)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "" smd rect
		(at 1 0 180)
		(size 0.3 0.4)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "A" smd rect
		(at 0.96 0)
		(size 0.48 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C" smd rect
		(at -0.96 0)
		(size 0.48 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "G" smd custom
		(at 0 -0.815)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.45 -0.185) (xy 0.45 -0.185) (xy 0.45 -0.435) (xy 1.2 -0.435) (xy 1.2 0.235) (xy -1 0.235)
					(xy -1.2 0.035) (xy -1.2 -0.435) (xy -0.45 -0.435)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "G" smd custom
		(at 0 0.815 180)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.45 -0.185) (xy 0.45 -0.185) (xy 0.45 -0.435) (xy 1.2 -0.435) (xy 1.2 0.035) (xy 1 0.235)
					(xy -1.2 0.235) (xy -1.2 -0.435) (xy -0.45 -0.435)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -1 -0.58) (xy 1.2 -0.58) (xy 1.2 -0.25) (xy 0.72 -0.25) (xy 0.72 0) (xy -0.72 0) (xy -0.72 -0.25)
				(xy -1.2 -0.25) (xy -1.2 -0.78)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -1 0.58) (xy 1.2 0.58) (xy 1.2 0.25) (xy 0.72 0.25) (xy 0.72 0) (xy -0.72 0) (xy -0.72 0.25)
				(xy -1.2 0.25) (xy -1.2 0.78)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/CoaxialSwitch_Hirose_MS-156C3_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
