(footprint "MMCX_Molex_73415-0961_Horizontal_1.6mm-PCB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex MMCX Horizontal Coaxial https://www.molex.com/pdm_docs/sd/734150961_sd.pdf")
	(tags "Molex MMCX Horizontal Coaxial")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "MMCX_Molex_73415-0961_Horizontal_1.6mm-PCB"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -3.75 1.75)
		(end 0.75 1.75)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 0.75 -1.75)
		(end -3.75 -1.75)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 0.75 1.75)
		(end 0.75 -1.75)
		(layer "Edge.Cuts")
	)
	(fp_text user "PCB edge"
		(at -3.35 0 90)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at -1.55 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 2.45 0)
		(size 2.6 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd custom
		(at 2.25 -1.525)
		(size 3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -1.5 -0.225) (xy -6 -0.225) (xy -6 -0.775) (xy -1.5 -0.775)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 2.25 1.525)
		(size 3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -1.5 0.775) (xy -6 0.775) (xy -6 0.225) (xy -1.5 0.225)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/MMCX_Molex_73415-0961_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
