(footprint "SMA_Amphenol_132134-10_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.amphenolrf.com/library/download/link/link_id/596219/parent/132134-10/")
	(tags "SMA SMD Female Jack Vertical")
	(property "Reference" "REF**"
		(at 0 -4.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "SMA_Amphenol_132134-10_Vertical"
		(at 0 4.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd circle
		(at 0 0 90)
		(size 1.73 1.73)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd custom
		(at 0 -2.8 180)
		(size 7.11 1.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -1.5 -1.42) (xy -1.36 -1.28) (xy -1.205 -1.155) (xy -1.035 -1.045) (xy -0.86 -0.95) (xy -0.675 -0.875)
					(xy -0.48 -0.82) (xy -0.28 -0.78) (xy -0.085 -0.765) (xy 0 -0.765) (xy 0 0.755) (xy -3.555 0.755)
					(xy -3.555 -1.595) (xy -1.645 -1.595)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 3.555 0.755) (xy 0 0.755) (xy 0 -0.765) (xy 0.085 -0.765) (xy 0.28 -0.78) (xy 0.48 -0.82) (xy 0.675 -0.875)
					(xy 0.86 -0.95) (xy 1.035 -1.045) (xy 1.205 -1.155) (xy 1.36 -1.28) (xy 1.5 -1.42) (xy 1.645 -1.595)
					(xy 3.555 -1.595)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 0 2.8)
		(size 7.11 1.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -1.5 -1.42) (xy -1.36 -1.28) (xy -1.205 -1.155) (xy -1.035 -1.045) (xy -0.86 -0.95) (xy -0.675 -0.875)
					(xy -0.48 -0.82) (xy -0.28 -0.78) (xy -0.085 -0.765) (xy 0 -0.765) (xy 0 0.755) (xy -3.555 0.755)
					(xy -3.555 -1.595) (xy -1.645 -1.595)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 3.555 0.755) (xy 0 0.755) (xy 0 -0.765) (xy 0.085 -0.765) (xy 0.28 -0.78) (xy 0.48 -0.82) (xy 0.675 -0.875)
					(xy 0.86 -0.95) (xy 1.035 -1.045) (xy 1.205 -1.155) (xy 1.36 -1.28) (xy 1.5 -1.42) (xy 1.645 -1.595)
					(xy 3.555 -1.595)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-10_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
