(footprint "SMA_Amphenol_132289_EdgeMount"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.amphenolrf.com/library/download/link/link_id/595984/parent/132289/")
	(tags "SMA")
	(property "Reference" "REF**"
		(at -3.96 -3 90)
		(layer "F.SilkS")
	)
	(property "Value" "SMA_Amphenol_132289_EdgeMount"
		(at 5 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 4.79 0 270)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 0 0 90)
		(size 1.5 5.08)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 -4.25 90)
		(size 1.5 5.08)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 -4.25 90)
		(size 1.5 5.08)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "2" smd rect
		(at 0 4.25 90)
		(size 1.5 5.08)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 4.25 90)
		(size 1.5 5.08)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
