(footprint "SMA_Amphenol_901-143_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Amphenol RF 901-143 https://www.amphenolrf.com/library/download/link/link_id/593645/parent/901-143/")
	(tags "SMA THT Female Jack Horizontal")
	(property "Reference" "REF**"
		(at -5.2 0 90)
		(layer "F.SilkS")
	)
	(property "Value" "SMA_Amphenol_901-143_Horizontal"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_line
		(start 4.3 -4.5)
		(end -4.3 -4.5)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(roundrect_rratio 0.087)
	)
	(pad "2" thru_hole circle
		(at -2.54 -2.54)
		(size 2.5 2.5)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "2" thru_hole circle
		(at -2.54 2.54)
		(size 2.5 2.5)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "2" thru_hole circle
		(at 2.54 -2.54)
		(size 2.5 2.5)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "2" thru_hole circle
		(at 2.54 2.54)
		(size 2.5 2.5)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-143_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
