(footprint "SMA_BAT_Wireless_BWSMA-KWE-Z001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "BAT Wireless BWSMA-KWE-Z00 https://www.lcsc.com/datasheet/lcsc_datasheet_2310171703_BAT-WIRELESS-BWSMA-KWE-Z001_C496551.pdf")
	(tags "SMA THT Female Jack Horizontal")
	(property "Reference" "REF**"
		(at -5.2 0 90)
		(layer "F.SilkS")
	)
	(property "Value" "SMA_BAT_Wireless_BWSMA-KWE-Z001"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.3 2.3)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(roundrect_rratio 0.087)
	)
	(pad "2" thru_hole circle
		(at -2.55 -2.55)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "2" thru_hole circle
		(at -2.55 2.55)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "2" thru_hole circle
		(at 2.55 -2.55)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(pad "2" thru_hole circle
		(at 2.55 2.55)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_BAT_Wireless_BWSMA-KWE-Z001.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
