(footprint "SMA_Molex_73251-1153_EdgeMount_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
	(tags "sma edge")
	(property "Reference" "REF**"
		(at -1.5 7 0)
		(layer "F.SilkS")
	)
	(property "Value" "SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(at -1.72 -7.11 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -1.5 7 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.72 0)
		(size 5.08 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.72 -4.38)
		(size 5.08 2.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.72 -4.38)
		(size 5.08 2.42)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "2" smd rect
		(at -1.72 4.38)
		(size 5.08 2.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.72 4.38)
		(size 5.08 2.42)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "2" smd rect
		(at 1.27 -4.38)
		(size 0.95 0.46)
		(layers "F.Cu")
	)
	(pad "2" smd rect
		(at 1.27 -4.38)
		(size 0.95 0.46)
		(layers "B.Cu")
	)
	(pad "2" smd rect
		(at 1.27 4.38)
		(size 0.95 0.46)
		(layers "F.Cu")
	)
	(pad "2" smd rect
		(at 1.27 4.38)
		(size 0.95 0.46)
		(layers "B.Cu")
	)
	(pad "2" thru_hole circle
		(at 1.72 -4.38)
		(size 0.97 0.97)
		(drill 0.46)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.72 4.38)
		(size 0.97 0.97)
		(drill 0.46)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
