(footprint "SMA_Molex_73251-2120_EdgeMount_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex SMA RF Connector, Edge Mount, (http://www.molex.com/pdm_docs/sd/732512120_sd.pdf)")
	(tags "sma edge")
	(property "Reference" "REF**"
		(at -0.705 -6.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "SMA_Molex_73251-2120_EdgeMount_Horizontal"
		(at -0.1 6.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 2.155 0 270)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 9.095 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.25 0)
		(size 3.69 1.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1404494382)
	)
	(pad "2" thru_hole circle
		(at -2.985 -3.4925)
		(size 0.97 0.97)
		(drill 0.46)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -2.985 3.4925)
		(size 0.97 0.97)
		(drill 0.46)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "2" smd roundrect
		(at -0.25 -3.4925)
		(size 3.69 2.665)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.09380863039)
	)
	(pad "2" smd roundrect
		(at -0.25 -3.4925)
		(size 3.69 2.665)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.09380863039)
	)
	(pad "2" smd roundrect
		(at -0.25 3.4925)
		(size 3.69 2.665)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.09380863039)
	)
	(pad "2" smd roundrect
		(at -0.25 3.4925)
		(size 3.69 2.665)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.09380863039)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-2120_EdgeMount_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
